Mesh the domain and assign material parameters

Apply load under certain boundary conditions

Is the Mohr-Coulomb failure criterion with a tensile cutoff satisfied?

Generate new cracks along element edges

Yes

End

Start

No

Is the specified time step reached?

Yes

No

Compute stress, strain and mechanical contact

Yes

No

**Figure 1.** Computing process of the proposed RDFA method